**Speed sensor module**

# API

|  |  |
| --- | --- |
| API | Usage |
| Void SpeedSen\_Init() | This API takes pointer to the configuration container of the Speed sensor driver to initialize the configured pins |
| Uint8 SpeedSen\_Read(void) | This API used to read the speed after conversions and calculations |

## Typedef

|  |  |
| --- | --- |
| Typedef | usage |
| SpeedSen\_ChannelType | Used to select the pin connected to the sensor |
| SpeedSen\_unit | Used to select the measuring unit miles or Km |